Last saved by: TO

NX-5200, NX-5300, NX-5400, NX-5700, NX-5800, NX-5900

Checksum: 3252
Version: 2.40

SN: B7C~

•	Added DMR feature enhancements. See Product Bulletin P17-10LM.
•	Also see product bulletin P17-30LM.
•	See release info for DMR Auto Slot Select Supplement Document V1.0 included in zip file.
•	Requires KPG-D1N Version 2.40 or higher.
•	Improvements for some issues including Lock Up problems.
•	Important note: NX‐5300 K5, K6, F5, and F6 only: If the Firmware was previously upgraded to Version K2.00 DMR High Deviation alignment is necessary. See Service Bulletin LSB-0353.
•	Before authenticating KWD-5300CV, please make sure the radio is using Firmware Version K2.01 or higher.
•	Adds New Features such as Multi RF Deck and More.
•	See Product Bulletins P-15-13LM and P-15-14LM.
•	This firmware upgrade is NOT eligible for warranty compensation.

Released December 2017